10:59:39 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3192.63 MHz, Windows 10 x64 found.
10:59:39 : [Hint] Recommend 32-bit Windows XP for a best work!
10:59:39 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
10:59:39 : API access enabled, device #0
2020-06-12
10:59:39 : Press F1 to About/HELP
10:59:39 : Get drive passport... OK
10:59:39 : Model: Fanxiang S101/128GB; Capacity: 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
10:59:53 : Program terminated.
11:00:38 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3193.96 MHz, Windows 10 x64 found.
11:00:38 : [Hint] Recommend 32-bit Windows XP for a best work!
11:00:38 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
11:00:38 : API access enabled, device #0
2020-06-12
11:00:38 : Press F1 to About/HELP
11:00:39 : Get drive passport... OK
11:00:39 : Model: Fanxiang S101/128GB; Capacity: 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
11:00:47 : Chinese
11:00:51 : Program terminated.
11:07:34 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3194.78 MHz, Windows 10 x64 found.
11:07:34 : [Hint] Recommend 32-bit Windows XP for a best work!
11:07:34 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
11:07:34 : API access enabled, device #0
2020-06-12
11:07:34 : Press F1 to About/HELP
11:07:34 : Get drive passport... OK
11:07:34 : Model: Fanxiang S101/128GB; Capacity: 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
11:07:40 : Get S.M.A.R.T. command... OK
11:07:40 : SMART status = GOOD
2020-06-12
11:07:59 : English
11:08:19 : Get drive passport... OK
11:08:19 : Model: Fanxiang S101/128GB; Capacity 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
11:08:21 : Get drive passport... OK
11:08:22 : Get S.M.A.R.T. Log directory... OK.
11:10:02 : Get S.M.A.R.T. command... OK
11:10:02 : SMART status = GOOD
11:10:19 : Program terminated.
11:10:27 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3195.24 MHz, Windows 10 x64 found.
11:10:27 : [Hint] Recommend 32-bit Windows XP for a best work!
11:10:27 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
11:10:27 : API access enabled, device #0
2020-06-12
11:10:27 : Press F1 to About/HELP
11:10:27 : Get drive passport... OK
11:10:27 : Model: Fanxiang S101/128GB; Capacity: 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
11:10:54 : Get drive passport... OK
11:10:54 : Get S.M.A.R.T. Log directory... OK.
11:11:03 : Chinese
11:11:06 : Get S.M.A.R.T. command... OK
11:11:06 : SMART status = GOOD
11:11:20 : Get S.M.A.R.T. command... OK
11:11:20 : SMART status = GOOD
11:11:28 : 获取驱动器通行证... OK
11:11:28 : Get S.M.A.R.T. Log directory... OK.
11:11:43 : Get S.M.A.R.T. command... OK
11:11:43 : SMART status = GOOD
11:11:51 : 获取驱动器通行证... OK
11:11:51 : Get S.M.A.R.T. Log directory... OK.
11:13:27 : Program terminated.
11:13:34 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3192.68 MHz, Windows 10 x64 found.
11:13:34 : [Hint] Recommend 32-bit Windows XP for a best work!
11:13:34 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
11:13:34 : API access enabled, device #0
2020-06-12
11:13:34 : Press F1 to About/HELP
11:13:34 : Get drive passport... OK
11:13:34 : Model: Fanxiang S101/128GB; Capacity: 250069680 LBAs; SN: AA000000000000002012; FW: S0128A
11:13:53 : English
11:14:41 : Chinese
11:14:56 : Program terminated.
09:09:05 : Starting Victoria 5.23 HDD/SSD. 8xCPU, 3600.28 MHz, Windows 7 x64 found.
09:09:05 : [Hint] Recommend 32-bit Windows XP for a best work!
09:09:05 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
09:09:05 : API access enabled, device #0
2020-12-23
09:09:06 : Press F1 to About/HELP
18:44:37 : Starting Victoria 5.23 HDD/SSD. 12xCPU, 3194.94 MHz, Windows 10 x64 found.
18:44:37 : [Hint] Recommend 32-bit Windows XP for a best work!
18:44:37 : Warning! Windows x64 detected! PIO mode supported on Windows x86 only.
18:44:37 : API access enabled, device #0
2020/12/24
18:44:37 : Press F1 to About/HELP
